{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Circular Section","Rectangular Section "],"not_rendered":{"charts":0,"images":10,"macros":1,"external_links":0,"defined_names":1,"comments":2,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Circular Section","index":0,"n_rows":56,"n_cols":28,"rows_kept":56,"cut":false,"hidden":false,"merged":[[46,2,46,3],[48,1,49,7]]}
[]
[null,null,null,null,"Circular Section Modeller for VecTor 5"]
[]
[null,"Hoop Reinforcement",null,null,null,null,"Main Reinforcement",null,null,null,null,null,"VecTor5 Input"]
[null,null,null,null,null,null,null,null,null,null,null,null,"Concrete Layers"]
[null,"Area (mm2)",null,null,100,null,"Area (mm2)",null,500,null,null,null,"MT","Dc (mm)","Wc (mm)","Rho-t (%)","Rho-z (%)","Nx"]
[null,"Spacing (mm)",null,null,100,null,"# of Bars",null,25,null,null,null,1,15,133.32,0,0,1]
[null,"Est (MPa)",null,null,200000,null,"Grade",null,null,null,null,null,1,15,227.98,0,0,1]
[null,null,null,null,null,null,"Es (MPa)",null,200000,null,null,null,1,18,301.06,0.33300000000000002,0.33300000000000002,1]
[null,"Clear Cover",null,null,null,null,"Fy(MPa)",null,400,null,null,null,1,18,355.96,0.33300000000000002,0.33300000000000002,1]
[null,null,null,null,null,null,"Fu(Mpa)",null,540,null,null,null,1,18,400.24,0.33300000000000002,0.33300000000000002,1]
[null,"Dimension (mm)",null,null,30,null,"esh (x10-3)",null,8,null,null,null,1,18,437.13,0.33300000000000002,0.33300000000000002,1]
[null,"# of Clear Cover Layers",null,null,2,null,"eu (x10-3)",null,80,null,null,null,1,18,468.37,0.33300000000000002,0.33300000000000002,1]
[null,null,null,null,null,null,"Dep (10-3)",null,0,null,null,null,1,18,495.05,0.33300000000000002,0.33300000000000002,1]
[null,"Cross Section",null,null,null,null,null,null,null,null,null,null,1,18,517.87,0.33300000000000002,0.33300000000000002,1]
[null,null,null,null,null,null,null,null,null,null,null,null,1,18,537.32000000000005,0.33300000000000002,0.33300000000000002,1]
[null,"Diameter (mm)",null,null,600,null,null,null,null,null,null,null,1,18,553.75,0.33300000000000002,0.33300000000000002,1]
[null,"# of Core Layers",null,null,30,null,null,null,null,null,null,null,1,18,567.42999999999995,0.33300000000000002,0.33300000000000002,1]
[null,"Member Type",null,null,1,null,null,null,null,null,null,null,1,18,578.54999999999995,0.33300000000000002,0.33300000000000002,1]
[null,null,null,null,null,null,null,null,null,null,null,null,1,18,587.26,0.33300000000000002,0.33300000000000002,1]
[null,null,null,null,null,null,null,null,null,null,null,null,1,18,593.66,0.33300000000000002,0.33300000000000002,1]
[null,null,null,null,null,null,null,null,null,null,null,null,1,18,597.83000000000004,0.33300000000000002,0.33300000000000002,1]
[null,null,null,null,null,null,null,null,null,null,null,null,1,18,599.80999999999995,0.33300000000000002,0.33300000000000002,1]
[null,null,null,null,null,null,null,null,null,null,null,null,1,18,599.63,0.33300000000000002,0.33300000000000002,1]
[null,null,null,null,null,null,null,null,null,null,null,null,1,18,597.29,0.33300000000000002,0.33300000000000002,1]
[null,null,null,null,null,null,null,null,null,null,null,null,1,18,592.75,0.33300000000000002,0.33300000000000002,1]
[null,null,null,null,null,null,null,null,null,null,null,null,1,18,585.97,0.33300000000000002,0.33300000000000002,1]
[null,null,null,null,null,null,null,null,null,null,null,null,1,18,576.87,0.33300000000000002,0.33300000000000002,1]
[null,null,null,null,null,null,null,null,null,null,null,null,1,18,565.33000000000004,0.33300000000000002,0.33300000000000002,1]
[null,null,null,null,null,null,null,null,null,null,null,null,1,18,551.21,0.33300000000000002,0.33300000000000002,1]
[null,null,null,null,null,null,null,null,null,null,null,null,1,18,534.29,0.33300000000000002,0.33300000000000002,1]
[null,null,null,null,null,null,null,null,null,null,null,null,1,18,514.30999999999995,0.33300000000000002,0.33300000000000002,1]
[null,null,null,null,null,null,null,null,null,null,null,null,1,18,490.89,0.33300000000000002,0.33300000000000002,1]
[null,null,null,null,null,null,null,null,null,null,null,null,1,18,463.51,0.33300000000000002,0.33300000000000002,1]
[null,null,null,null,null,null,null,null,null,null,null,null,1,18,431.41,0.33300000000000002,0.33300000000000002,1]
[null,null,null,null,null,null,null,null,null,null,null,null,1,18,393.43,0.33300000000000002,0.33300000000000002,1]
[null,null,null,null,null,null,null,null,null,null,null,null,1,18,347.68,0.33300000000000002,0.33300000000000002,1]
[null,null,null,null,null,null,null,null,null,null,null,null,1,18,290.47000000000003,0.33300000000000002,0.33300000000000002,1]
[null,null,null,null,null,null,null,null,null,null,null,null,1,15,227.98,0,0,1]
[null,null,null,null,null,null,null,null,null,null,null,null,1,15,133.32,0,0,1]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,"Rebar Layers"]
[null,null,null,null,null,null,null,null,null,null,null,null,"MT","N","Ys (mm)","As (mm2)","Db (mm)","Fy (MPa)","Fu (MPa)","Es (MPa)","esh (me)","eu (me)","Dep (me)","L/Db",null,"n","rb","Buckling Effects"]
[null,null,null,null,null,null,null,null,null,null,null,null,1,1,53.89,500,25.23,400,540,200000,8,80,0,7.93,null,2,15.853309190424044,"Small"]
[null,null,null,null,null,null,null,null,null,null,null,null,1,2,62.02,1000,25.23,400,540,200000,8,80,0,7.93,null,2,15.853309190424044,"Small"]
[null,null,null,null,null,null,null,null,null,null,null,null,1,3,85.9,1000,25.23,400,540,200000,8,80,0,7.93,null,2,15.853309190424044,"Small"]
[null,null,null,null,null,null,null,null,null,null,null,null,1,4,124.02,1000,25.23,400,540,200000,8,80,0,7.93,null,2,15.853309190424044,"Small"]
[null,null,null,null,null,null,null,null,null,null,null,null,1,5,173.99,1000,25.23,400,540,200000,8,80,0,7.93,null,2,15.853309190424044,"Small"]
[null,"This spreadsheet is programmed by Rafael Salgado as a part of a project supervised by Dr. Serhan Guner.",null,null,null,null,null,null,null,null,null,null,1,6,232.67,1000,25.23,400,540,200000,8,80,0,7.93,null,2,15.853309190424044,"Small"]
[null,null,null,null,null,null,null,null,null,null,null,null,1,7,296.37,1000,25.23,400,540,200000,8,80,0,7.93,null,2,15.853309190424044,"Small"]
[null,null,null,null,null,null,null,null,null,null,null,null,1,8,335.86,1000,25.23,400,540,200000,8,80,0,7.93,null,2,15.853309190424044,"Small"]
[null,"Copyright © 2014 ",null,null,null,null,null,null,null,null,null,null,1,9,397.54,1000,25.23,400,540,200000,8,80,0,7.93,null,2,15.853309190424044,"Small"]
[null,"Version 1.0",null,null,null,null,null,null,null,null,null,null,1,10,452.3,1000,25.23,400,540,200000,8,80,0,7.93,null,2,15.853309190424044,"Small"]
[null,null,null,null,null,null,null,null,null,null,null,null,1,11,496.69,1000,25.23,400,540,200000,8,80,0,7.93,null,2,15.853309190424044,"Small"]
[null,null,null,null,null,null,null,null,null,null,null,null,1,12,527.94000000000005,1000,25.23,400,540,200000,8,80,0,7.93,null,2,15.853309190424044,"Small"]
[null,null,null,null,null,null,null,null,null,null,null,null,1,13,544.05999999999995,1000,25.23,400,540,200000,8,80,0,7.93,null,2,15.853309190424044,"Small"]

{"sheet":"Rectangular Section ","index":1,"n_rows":68,"n_cols":28,"rows_kept":68,"cut":false,"hidden":false,"merged":[[61,2,61,3],[63,1,64,7]]}
[]
[null,null,null,null,"Rectangular and Slab Section Modeller for VecTor 5"]
[]
[null,"Shear Reinforcement",null,null,null,null,"Main Reinforcement",null,null,null,null,null,"VecTor5 Input"]
[null,null,null,null,null,null,null,null,null,null,null,null,"Concrete Layers"]
[null,"Area (mm2)",null,null,100,null,"Area (mm2)",null,500,null,null,null,"MT","Dc (mm)","Wc (mm)","Rho-t (%)","Rho-z (%)","Nx"]
[null,"Spacing (mm)",null,null,100,null,"Grade",null,null,null,null,null,1,15,400,0,0,1]
[null,"Est (MPa)",null,null,200000,null,"Es (MPa)",null,200000,null,null,null,1,15,400,0,0,1]
[null,null,null,null,null,null,"Fy (MPa)",null,400,null,null,null,1,17.419,400,0.5,0.55555555555555558,1]
[null,"Horizontal Direction",null,null,null,null,"Fu (MPa)",null,540,null,null,null,1,17.419,400,0.5,0.55555555555555558,1]
[null,null,null,null,null,null,"esh (x10-3)",null,8,null,null,null,1,17.419,400,0.5,0.55555555555555558,1]
[null,"Dimension (mm)",null,null,400,null,"eu (x10-3)",null,80,null,null,null,1,17.419,400,0.5,0.55555555555555558,1]
[null,"# of bars",null,null,4,null,"Dep (x10-3)",null,0,null,null,null,1,17.419,400,0.5,0.55555555555555558,1]
[null,"# of cross ties",null,null,1,null,null,null,null,null," ",null,1,17.419,400,0.5,0.55555555555555558,1]
[null,null,null,null,null,null,"Cross Section",null,null,null,null,null,1,17.419,400,0.5,0.55555555555555558,1]
[null,"Vertical Direction",null,null,null,null,null,null,null,null,null,null,1,17.419,400,0.5,0.55555555555555558,1]
[null,null,null,null,null,null,"Clear Cover (mm)",null,30,null,null,null,1,17.419,400,0.5,0.55555555555555558,1]
[null,"Dimension (mm)",null,null,600,null,"# Clear Cover Layers",null,2,null,null,null,1,17.419,400,0.5,0.55555555555555558,1]
[null,"# of bars",null,null,3,null,"# Core Layers",null,31,null,null,null,1,17.419,400,0.5,0.55555555555555558,1]
[null,"# of cross ties",null,null,0,null,"Member Type",null,1,null,null,null,1,17.419,400,0.5,0.55555555555555558,1]
[null,null,null,null,null,null,null,null,null,null,null,null,1,17.419,400,0.5,0.55555555555555558,1]
[null,null,null,null,null,null,null,null,null,null,null,null,1,17.419,400,0.5,0.55555555555555558,1]
[null,null,null,null,null,null,null,null,null,null,null,null,1,17.419,400,0.5,0.55555555555555558,1]
[null,null,null,null,null,null,null,null,null,null,null,null,1,17.419,400,0.5,0.55555555555555558,1]
[null,null,null,null,null,null,null,null,null,null,null,null,1,17.419,400,0.5,0.55555555555555558,1]
[null,null,null,null,null,null,null,null,null,null,null,null,1,17.419,400,0.5,0.55555555555555558,1]
[null,null,null,null,null,null,null,null,null,null,null,null,1,17.419,400,0.5,0.55555555555555558,1]
[null,null,null,null,null,null,null,null,null,null,null,null,1,17.419,400,0.5,0.55555555555555558,1]
[null,null,null,null,null,null,null,null,null,null,null,null,1,17.419,400,0.5,0.55555555555555558,1]
[null,null,null,null,null,null,null,null,null,null,null,null,1,17.419,400,0.5,0.55555555555555558,1]
[null,null,null,null,null,null,null,null,null,null,null,null,1,17.419,400,0.5,0.55555555555555558,1]
[null,null,null,null,null,null,null,null,null,null,null,null,1,17.419,400,0.5,0.55555555555555558,1]
[null,null,null,null,null,null,null,null,null,null,null,null,1,17.419,400,0.5,0.55555555555555558,1]
[null,null,null,null,null,null,null,null,null,null,null,null,1,17.419,400,0.5,0.55555555555555558,1]
[null,null,null,null,null,null,null,null,null,null,null,null,1,17.419,400,0.5,0.55555555555555558,1]
[null,null,null,null,null,null,null,null,null,null,null,null,1,17.419,400,0.5,0.55555555555555558,1]
[null,null,null,null,null,null,null,null,null,null,null,null,1,17.419,400,0.5,0.55555555555555558,1]
[null,null,null,null,null,null,null,null,null,null,null,null,1,17.419,400,0.5,0.55555555555555558,1]
[null,null,null,null,null,null,null,null,null,null,null,null,1,17.419,400,0.5,0.55555555555555558,1]
[null,null,null,null,null,null,null,null,null,null,null,null,1,15,400,0,0,1]
[null,null,null,null,null,null,null,null,null,null,null,null,1,15,400,0,0,1]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,"Rebar Layers"]
[null,null,null,null,null,null,null,null,null,null,null,null,"MT","N","Ys (mm)","As (mm2)","Db (mm)","Fy (MPa)","Fu (MPa)","Es (MPa)","esh (me)","eu (me)","Dep (me)","L/Db",null,"n","rb","Buckling Effects"]
[null,null,null,null,null,null,null,null,null,null,null,null,1,1,53.899454281055924,2000,25.231325220201601,400,540,200000,8,80,0,11.89,null,3,23.779963785636067,"High"]
[null,null,null,null,null,null,null,null,null,null,null,null,1,2,300,1000,25.231325220201601,400,540,200000,8,80,0,15.85,null,4,31.706618380848088,"High"]
[null,null,null,null,null,null,null,null,null,null,null,null,1,3,546.10054571894409,2000,25.231325220201601,400,540,200000,8,80,0,11.89,null,3,23.779963785636067,"High"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"This spreadsheet is programmed by Rafael Salgado as a part of a project supervised by Dr. Serhan Guner."]
[]
[]
[null,"Copyright © 2015"]
[null,"Version 1.1"]